Conclusion Heating Control

If you want to Scale an analogue input you have to address the input as an periphery input so expect for IW752 you write PIW752.